**CHECKLIST – NECESSARY SAFETY PRECAUTIONS SAMPLE**

"DO NOT CUT, WELD, OR USE OTHER OPEN-FLAME OR ABRASIVE SPARK-PRODUCING EQUIPMENT UNTIL THE FOLLOWING PRECAUTIONS HAVE BEEN TAKEN."

Check Each Item:

 Owner/Contractor

 \_\_\_\_\_\_\_\_\_\_1.The location where the work is

 to be done has been personally

 examined.

 \_\_\_\_\_\_\_\_\_\_A.Sprinklers, where provided,

 are in commission and will not

 be taken out of service until

 this work has been completed.

 (Coordination with plant may be

 required.)

 \_\_\_\_\_\_\_\_\_\_B.There is no flammable or

 combustible lint, dust, vapors

 and liquids on unpurged tanks or

 equipment previously containing

 such materials in the area.

 (Obtain Confined Space Entry

 Permit.)

 \_\_\_\_\_\_\_\_\_\_C.This work will be confined to

 the area or equipment specified

 in the permit.

 2.The following safeguards have been

 provided:

 \_\_\_\_\_\_\_\_\_\_A.Floors and surroundings have been

 swept clean and have been wet

 down.

 \_\_\_\_\_\_\_\_\_\_B.Ample portable extinguishing

 equipment -- hand hoses,

 extinguishers, water pails, etc.

 -- have been provided.

 \_\_\_\_\_\_\_\_\_\_C.Ample ventilation to remove

 smoke/vapor from work area.

 3.If the work involves "HOT WORK," the

 following additional safeguards shall

 be provided.

 \_\_\_\_\_\_\_\_\_\_A.All portable combustibles have

 been relocated 40 ft. from the

 operation and the remainder

 protected with metal guards or

 flameproofed covers (not ordinary

 tarpaulins).

 \_\_\_\_\_\_\_\_\_\_B.All floor and wall openings

 within 40 ft. of the operations

 have been tightly covered.

 \_\_\_\_\_\_\_\_\_\_C.Responsible employees have been

 assigned to watch for dangerous

 sparks in the area.

 \_\_\_\_\_\_\_\_\_\_D.Check area for smoke or heat

 detector(s), if found see 1 A

 for action.

 \_\_\_\_\_\_\_\_\_\_4.Flame or spark-producing equipment to

 be used has been inspected and found

 in good repair.

 \_\_\_\_\_\_\_\_\_\_5.Arrangements have been made for a

 patrol of the area, including floors

 above and below, during any lunch or

 rest period for a sufficient time

 after work has been completed.

 Y -- Yes

 N -- No

 N/A -- Not Applicable