**CHECKLIST – NECESSARY SAFETY PRECAUTIONS SAMPLE**

"DO NOT CUT, WELD, OR USE OTHER OPEN-FLAME OR ABRASIVE SPARK-PRODUCING EQUIPMENT UNTIL THE FOLLOWING PRECAUTIONS HAVE BEEN TAKEN."

Check Each Item:

Owner/Contractor

\_\_\_\_\_\_\_\_\_\_1.The location where the work is

to be done has been personally

examined.

\_\_\_\_\_\_\_\_\_\_A.Sprinklers, where provided,

are in commission and will not

be taken out of service until

this work has been completed.

(Coordination with plant may be

required.)

\_\_\_\_\_\_\_\_\_\_B.There is no flammable or

combustible lint, dust, vapors

and liquids on unpurged tanks or

equipment previously containing

such materials in the area.

(Obtain Confined Space Entry

Permit.)

\_\_\_\_\_\_\_\_\_\_C.This work will be confined to

the area or equipment specified

in the permit.

2.The following safeguards have been

provided:

\_\_\_\_\_\_\_\_\_\_A.Floors and surroundings have been

swept clean and have been wet

down.

\_\_\_\_\_\_\_\_\_\_B.Ample portable extinguishing

equipment -- hand hoses,

extinguishers, water pails, etc.

-- have been provided.

\_\_\_\_\_\_\_\_\_\_C.Ample ventilation to remove

smoke/vapor from work area.

3.If the work involves "HOT WORK," the

following additional safeguards shall

be provided.

\_\_\_\_\_\_\_\_\_\_A.All portable combustibles have

been relocated 40 ft. from the

operation and the remainder

protected with metal guards or

flameproofed covers (not ordinary

tarpaulins).

\_\_\_\_\_\_\_\_\_\_B.All floor and wall openings

within 40 ft. of the operations

have been tightly covered.

\_\_\_\_\_\_\_\_\_\_C.Responsible employees have been

assigned to watch for dangerous

sparks in the area.

\_\_\_\_\_\_\_\_\_\_D.Check area for smoke or heat

detector(s), if found see 1 A

for action.

\_\_\_\_\_\_\_\_\_\_4.Flame or spark-producing equipment to

be used has been inspected and found

in good repair.

\_\_\_\_\_\_\_\_\_\_5.Arrangements have been made for a

patrol of the area, including floors

above and below, during any lunch or

rest period for a sufficient time

after work has been completed.

Y -- Yes

N -- No

N/A -- Not Applicable